The files in this directory is kindly contributed by 
Joachim Jansen <jj@ekf.de> as an example of RS274D with
an separate aperture file.

Please note that these files should NOT work with gerbv since they
are RS274D and not RS274X.

	l1.off  : The Gerber file
	ekf.gap : D-code table maintained by CAM350

$Id$
