G04 Test flashing of rectangular apertures*
G04 Four groups of rectangular apertures are arranged in a square*
G04 Handcoded by Julian Lamb *
%MOIN*%
%FSLAX23Y23*%
%ADD10R,0.050X0.080*%
%ADD11R,0.080X0.050X0.025*%
%ADD12R,0.050X0.025X0.025X0.0150*%

G04 No hole, centered at 0,0 *
G54D10*
X0Y0D03*

G04 Round hole, centered at 0.1,0 *
G54D11*
X00100Y0D03*

G04 Square hole, centered at 0,0.1 *
G54D12*
X0Y00100D03*

G04 Two, with round holes, slightly overlapping, centered at 0.1,0.1 *
G54D11*
X00100Y00090D03*
X00100Y00110D03*

M02*
